2025 Kenworth T880 Dump Trucks

**\*\*NOTE: If vendors choose to not comply with certain specifications listed. Those exceptions must be identified and documented on a separate sheet and uploaded as part of the vendors response.**

Unless otherwise specified in this Invitation to Bid (ITB), reference to a specific manufacturer or a specific product or model in the bid specifications does not restrict bidders to that manufacturer, product or model.  This method is used to indicate the functional requirements (e.g., type, design, characteristics, quality) of the article desired.  Bids may be considered on other manufacturers’ products or other models determined by the Purchasing Division to be the functional equivalent of the product or model referenced.

**VEHICLE CONFIGURATION: Vendor Complies \_\_\_\_\_ YES \_\_\_\_\_ NO**

* NEW 2025 T880 CHASSIS
* CUMMINS X15 500V/1850 ENGINE
* 1850 ENGINE
* ALLISON 4500RDS TRANS
* 206 FRONT STEER AXLE
* 40K REAR DANA AXLES

**WATER TANK:** **Vendor Complies \_\_\_\_\_ YES \_\_\_\_\_ NO**

* SCHLOTH & DOWNEY 15’ DUMP BODY W/AIR AND ELECTRIC END OF FRAME